4.6.5. REP mode – Repetitive insertion of components<br>

### 4.6.5. REP mode – Repetitive insertion of components

Repetitive insertion mode is useful when editing both the plan of the building and the installation. The REP mode is designed to facilitate inserting of components of the same type.

Blue REP letters in the field indicate REP mode activated. Grey letters mean that the REP mode is disabled.

When this mode is activated, components of the selected type are inserted until the right mouse button is pressed (after inserting a component, the mode of inserting that component is still activated). When REP mode is disabled, after inserting a component the mode of selecting components is activated.

The REP mode applies to structural, installation and fitting components (walls, windows, doors, radiator, heating floor, manifold, etc.).

¨ To enable or disable the REP mode:

- Click once on the REP field in the upper right corner of the screen.

or

- Press the Alt+B keys.