6.2.8. Polylines for depicting piping<br>

### 6.2.8. Polylines for depicting piping

Polylines for drawing pipe system is a graphical component designed to depict part or the whole of pipe system within a heating zone. Their properties are the same as those of an ordinary polyline. Piping can be drawn automatically or manually.

How this line can be used to draw pipe systems is explained in section 0. These components are only available on a “Plan view” type sheet in the “Floor heat. dwg.” layer in the “Radiant” tab.

Buttons on the “Radiant” toolbar:

Appearance on screen (plan view) (colours: red = supply, blue = return):

“Polylines for depicting piping” component data:

! Pair of polylines has specific data fields, which are used only when polylines are placed in the drawing and apply to their relative position and spacing. After placing a pair of polylines, each of them forms a separate component and has other fields in the table.

Fields used when placing a pair of polylines in the drawing:

Pipe spacing

Numerical field. Pipe spacing for a pair of polylines. When AUTO mode is enabled, the spacing is automatically adjusted to the value read from the results for the HZ.

Relative arrangement s/r

Relative arrangement of supply and return for a pair of polylines. When AUTO mode is enabled, the relative arrangement of lines is adjusted automatically depending on the situation on the drawing.

Fields displayed when marking a polyline drawn before:

Line style

Selection field. Select from list the appearance of the line or configure it – component appearance window is opened.