7.2.2. Configuring the appearance of radiator labels<br>

### 7.2.2. Configuring the appearance of radiator labels

A radiator label may be configured in two ways. It may be “attached” to the radiator, so that it cannot be moved in the drawing (to move such label, you have to change the appearance of the component). The appearance of the “Together with radiator” label in the drawing and in the configuration is as follows:

The label may also be placed in a separate frame, which can be moved freely in the drawing (this is useful when the radiator label is obscured by other components in the drawing). The appearance of the “In moving field” label in the drawing and in the configuration is as follows:

In the “Edit” tab you can define simplifications and scale of drawing simplifications during editing.