5.3.4. Complex cases encountered when editing construction<br>

### 5.3.4. Complex cases encountered when editing construction

Solutions to some more complex cases of editing building construction are presented in this section.

Varying thickness of a wall within one straight segment:

¨ To introduce wall thickness variation:

1. Enter each segment of different thickness as a separate wall type component and specify its thickness:

2. Move one of the walls so that the faces on one side of the walls form a straight line and ends of the walls coincide (after acquiring some skill it is possible to draw walls in this way right away; to do this you have to disable the AUTO mode, so that wall ends are not connected automatically):

3. Insert an additional wall segment to join the ends of walls of different thickness:

In a similar way you can join 3 walls, of which the two collinear walls are of different thickness. The result should, for instance, look like the one below:

It is easier to solve this case by defining the thicker collinear wall as an asymmetrical wall: