3.4.3. “Default types” tab<br>

### 3.4.3. “Default types” tab

In the “Default types” tab you can specify default types of system components, which will be selected from catalogues in the project. These include:

- “Default pipe type”.

- “Default pipe insulation type”.

- “Default manner of assembling cross-pieces”.

- “Default type on non-integrated radiators”.

- “Default type on integrated radiators”.

- “Default system of connections”.

- “Default valve type on supply rad. circuit pipes”.

- “Default valve type on return rad. circuit pipes”.

- “Default catalogue for selecting valve heads”.

It is possible to specify two types of default connection systems: for integrated and non-integrated radiators. Depending on pipe catalogue loaded into the project, the contents of both lists may be identical in part or it may be completely different. That depends on the pipe manufacturer and on radiator connections offered.

Here you also specify the “Default restrictions of radiator size”. When you click on the button, a window opens where you can enter the minimum and maximum height, length and depth of radiator. Minimum dimension for radiator enclosure can also be specified.