C.5. Appending subsequent fragments of the base drawing<br>

C.5. Appending subsequent fragments of the base drawing

To proceed with appending subsequent fragments of the base drawing, click on the “Next” button in the upper right corner of the screen. The entire base drawing is displayed on the left side, while the fragment being appended is displayed on the right side. If you use the “navigator”, then the project status and position of the fragment being appended are displayed in the middle of the screen.

¨ To append the next fragment of the base drawing using the “navigator”:

1. Load or scan the next fragment of the base drawing. Make sure with the navigator (in the middle of the screen), which part is being appended.

2. Mark the same characteristic point on the entire drawing preview and on the fragment being appended. To see which point is expected – look at the “Mark point” frame. Points are marked with the RIGHT mouse button. In case of error you can change the setting in the “Mark point” frame and click again.

3. Mark the second characteristic point.

4. Mark the third characteristic point - this is required only when two sides of the part being appended adjoin the fragments of the base drawing already appended.

5. Click “Append”.

Append the subsequent fragments of the base drawing using the “navigator”. After appending all parts click “Next” to move to the last stage – trimming and scaling.

If the “navigator” is not enabled, then the procedure is similar to that described above, you only have to specify the “Append method” and “Append direction” for each fragment.