2.3.10. Analysis of complete results and printout<br>

### 2.3.10. Analysis of complete results and printout

After obtaining correct, errorless calculation results you should see the other results: installation parameters, general results including collective data and a list of manifolds for individual control circuits and bill of materials.

After clicking on the “Print” button a print preview is displayed together with a printout configuration window. The range of information to be printed is called print layout. To change it go to the “Layout” tab in the print preview window and select the appropriate layout. The list of layouts covers all applications of the program and some of them may not be applicable to floor heating. You can also create your own layouts -–this is described further in this manual.

You can print the plan view of the storey and the installation after reverting to the editor. Printout configuration is done in a special data table on the “Print” layer (tabs in the lower right part of the screen).

By default the program will not draw the pipe system within the heating zone. In cases when the information on pipe laying pattern is not sufficient for the fitter, the pipe pattern in the heating circuit may be drawn manually or automatically. To do this move to the “Draw FH loop” layer and select in the “Radiant” tab one of the components of the “Polylines representing pipe system” type , . The manner of using these components is described in sections 6.2.8 and 7.12.

Instead of printing the drawing on a printer or plotter you can export it to other CAD application. To do this use the “File / Export drawing” command and select one of the available formats.