2.6.1. Description of storeys<br>

### 2.6.1. Description of storeys

Description of storeys can be performed by the User by clicking on storey level on the building structure tree. On the right side of the screen a widow for storeys edition “Building structure: Storey”.

Edition fields are used for input of storey name, comment to the name and completion of data concerning its dimensions. That are: floor ordinate, height of storey in axes, floor thickness, window sill ordinate, default width of heater recess.

In building structure select a storey, towards which the floor ordinates on each floor will be calculated. For selected storey mark the field “Relation storey”. A floor ordinate for each storey is calculated by the program automatically on the basis of declared floor ordinate and storey height. Moreover, all storeys locates over related storey will have the ordinate with positive character and all storeys located underneath will have the ordinate with negative character.

The program can automatically complete the dimensions described above, because they have been declared in „Expression variables”. Their value should be controlled so as they could comply with building parameters.

Field concerning default heater recess width has to be still completed. Its declaring enables faster data edition of heater selection. More information to this can be found in chapter 4.5.1.

In field „Type” for actual storey are displayed for example „Ground floor”, „First floor”, „Cellar”. Selection can be made in this field or in pop-up menu concerning the storey.

The User can make its selection from a pop-up list in field „Type”. If it is a single-storey building, for the first and only building level it is assigned as “Ground floor”. If there is more storeys in the building, the User can select their type on the selection list. Selection of type “Ground floor” will cause, that all storeys above will have assigned type “Floor” and all storeys below – type “Ceiling”.

In the building structure tree the possibility of storey type selection is limited to „Ground floor” only. Such selection will cause assigning of adequate types to all storeys above and below the declared storey.