7.12.1. Automatic drawing<br>

### 7.12.1. Automatic drawing

To enable automatic drawing of the piping use the component. After selecting and moving to the HZ area, a cross is displayed, which indicates the connection point of pipe feeds to the HZ. In case of a “Spiral pipe pattern” specified in HZ data, you have to indicate the direction of pipe laying: an arrow is displayed, which indicates the direction and a preview of the piping is displayed.

In case of a “Double pipe meander pattern” click first at the point from which the drawing of the proper meander is to start, and then click at the point where drawing of a single loop is to end. After accepting the arrangement click on the HZ to insert the loops. An example of a double pipe meander pattern is shown below.