5.2.3. Opening in wall<br>

### 5.2.3. Opening in wall

The “Opening in wall” component cannot stand alone – it may only be placed on a wall to which it is assigned, and its data are displayed in the lower part of the wall data table. This is a graphical component and has no effect on calculations, in particular it does not eliminate partitioning of rooms by walls. To place an opening in a wall, select it from the “Components” toolbar and click on the wall axis at a selected point. You can move the opening along the wall.

Button on the “Components” toolbar:

Appearance on screen:

“Opening in wall” component data:

Width [m]

Numerical field. Width of opening along the axis of the wall.

Height [m]

Numerical field. Height of opening.

Draw line

Selection field. This field can be set to “Yes” or “No” and it applies to the manner of drawing. The “Yes” setting means that wall contour is drawn along opening