6.1.15. Mixer (temperature reducer)<br>

### 6.1.15. Mixer (temperature reducer)

This component represents a mixer (temperature reducer) used to connect floor heating systems.

Button on the “Central” toolbar:

Appearance on screen (plan / schematic view):

“Mixer” component data:

Symbol

Text field. Symbol that identifies the component unambiguously.

Mixer type

Selection field. Type of mixer. By default an arrangement of 3-way valve and pump is assumed as a mixer. You can indicate other type in the pull-down list.

Outlet temp.

Numerical field. Temperature at the outlet of mixer. The value may be determined automatically when the mixer feeds a radiant heating system (using information on connected circuits and manifolds of radiant heating system). You can specify a value or enter “?” to revert to automatic outlet temperature determination.

Component status

Selection field. Select from list the current status of component: existing or under design. Affects only bill of material.

ts/qs min. RH

Numerical field. Lower limit of temperature range for radiant heating. Value taken into account when optimising supply temperature.

ts/qs max. RH

Numerical field. Upper limit of temperature range for radiant heating. Value taken into account when optimising supply temperature.

After selecting mixer type, the table displays below the mixer data the data of existing valves and pump. Valve types must be specified.