2.4.8. Analysis of complete results and project printout<br>

### 2.4.8. Analysis of complete results and project printout

All calculation results are given in tables: “General results”, “Pipe-runs”, “Terminal units” and “Bills of materials”. The table of pipe-runs also provides information on valves and pumps and manifolds. The bill of materials is split into several parts. The contents of the tables may be specified (you may hide some columns). You can also look for components that meet defined conditions, e.g. pipe-runs of specified number, with medium velocity exceeding a set value, with water temperature drop higher than set, etc. Detailed description of tables of results and associated functions is given in further sections of this manual.

After clicking on the “Print” button, print preview is displayed with a window enabling convenient configuration of the scope and style of printout. To switch the print preview to another table of results, select the “Layout” tab in the control window and select the required layout. You can create your own layout.

Upon completing the printout go back to the results by clicking on the “End” button.

To go back to the graphical editor click on the “Editor” button in the upper part of the screen. In the graphical editor the results are:

- automatically displayed in the drawing, e.g. radiator and valve sizes,

- displayed in the drawing after adding additional graphical components (pipe-run diameters, flow rates in pipe-runs and some other results for pipe-runs).

To display sized diameters of pipes in the drawing you have to place “Pipe-run label” components from the “Graphics” tab on the pipe-runs. This component can be configured to display various results, e.g. pipe-run diameter, flow rate, insulation thickness. A configured pipe-run label can be saved to the user toolbar (“Append to toolbar”) for further use.

Other graphical components can be added to the drawing, e.g. a project chart. Such a chart can be configured in a broad range, and it can also be saved for further use.

Checking partial results of individual components of the system is possible with “bubbles”. When you position the mouse pointer over a component, a bubble appears with results of that component. When you position the mouse pointer over a junction (connection point of pipe-runs) the bubble displays information on the manner of implementing that junction using components available in catalogues.

Instead of printing on a printer or a plotter, you can export drawings into graphical files, including CAD type files. To do this use the “File / Export drawing...” command and select one of the available formats.

In the graphical editor you can also view the results in tabular form. To do this press the F11 function key or click on the “Calculation results” button in the “Program” toolbar.

To print tables select the appropriate item in the pop-up menu after clicking the right mouse button within the table.

Some tables include a (torch) icon. Clicking on this icon results in the indication in the drawing of the component to which the row in the table with the icon applies. Finding a component the other way round (in the table) is available by selecting appropriate command from the pop-up menu that appears upon right clicking the component in the drawing. If the table currently displayed does not include results of the component indicated in the drawing, the appropriate table is displayed.

Drawing printouts are configured in the “Printout” layer selected from among the tabs in the lower right part of the screen.