4.8.13. Repeated inserting of an identical component<br>

### 4.8.13. Repeated inserting of an identical component

By default, after placing a component or module, the basic operating mode of marking and moving is restored. Often, however, you will want to insert several components of the same type. In these cases it is convenient to use the “Insert last item” command, which is assigned to the F3 function key.

¨ To place another component or module of the same type after inserting the first one, select “Edit / Insert last item” (F3, ).

When inserting several identical components in sequence it is also possible to use the REP mode – repetitive insertion of components. When this mode is activated, components of the selected type are inserted until the right mouse button is pressed (after inserting a component, the mode of inserting that component is still activated). When REP mode is disabled, after inserting a component the mode of selecting components is activated.

The REP mode applies to structural, installation and fitting components (walls, windows, doors, radiator, heating floor, manifold, etc.).

¨ To enable or disable the REP mode:

- Click once on the REP field in the upper right corner of the screen.

or

- Press the Alt+B keys.

! The setting described above may be helpful when editing building structure with the use of “wall” components.