3.4.6. “Edit” tab<br>

### 3.4.6. “Edit” tab

The “Edit” tab presents the current data on sheet display and edit parameters:

- “Isometric / Support angle” – toggle on/off the defining of isometric view angle to which pipe-runs and polylines may be aligned. When drawing in isometric view is enabled then in addition to vertical and horizontal components, you can also place them inclined at the defined angle. Standard value of that angle is 30º.

- “Calculate elevations in isom.” – available only for “Schematic view” type sheets. Toggles on/off calculation of elevations in isometric view and specification of permissible angle deviation.

- “Radiator to floor distance [cm]” – distance from floor taken into account when inserting a radiator into a drawing in a “Schematic view” type sheet when AUTO mode is on.

- “Pipe-runs pair spacing [cm]” – distance applied when drawing a pair of pipe-runs in the sheet.

- “Pipe-runs length calculation” – specify whether the lengths of all pipe-runs in the drawing are to be calculated, only vertical pipe-runs (in a “Schematic view” sheet) or not calculated at all.

- “Auto radiator circuit pipes modification” - toggle on/off automatic modification of radiator circuit pipes between riser and radiator after changing type.

- “Horizontal and vertical grid” and “Snap to grid” – specify grid parameters, to which the components will be aligned. Each component that is inserted or moved is snapped to the grid.

- “Connecting distance with AUTO disabled” – distance at which pipe-runs will be automatically connected when AUTO mode is not on.

- “Find connection in AUTO mode” – distance at which the program looks for basic components or modules to be connected when AUTO mode is on.

- “Workspace size” – specify point of origin and size of workspace (drawing sheet).

- “Always show print layout” – toggle on / off display of page size and paper cutting lines in each layer. By default the page layout is shown only in the “Print” layer.