9.4. Results in graphical editor<br>

## 9.4. Results in graphical editor

After successful calculations the project achieves a “calculated” status. This is indicated by an icon on the left side of the status line, which, upon completing calculations, has the following appearance: .

Calculation results are saved to the project file and most of them may be printed or displayed in hints in the graphical editor. The calcualtion error list shown under tables of results and tables of results are also available in the graphical editor.

The results which can be shown on the system diagram and printed, may be grouped in two categories:

- results of calculations of pipe-runs (system segments) – not displayed by default; a “Pipe-run label” component is required on each pipe-run the results of which are to be displayed,

- results of calculations of receptors, fittings and possibly system junctions – displayed automatically; their configuration is required in the “Options/component appearance” menu. Empty sets of calculation results may be specified for some components by default.

Pipe-runs are not described automatically on drawings, as this could obscure other components in the drawing. The user can place labels on every pipe-run. It is also possible to place labels on a number of pipe-runs simultaneously. Labels can be placed when editing data (prior to calculations) or after completing calculations and reverting to the graphical editor.

¨ To place labels on multiple pipe-runs simultaneously:

- mark the appropriate pipe-runs using the functions for marking multiple components (see section: 4.8.3 – 4.8.6),

- double click one of the pipe-run labels in the “Graphics” tab,

- labels are placed in the middle of pipe-run, and if there are many of them, it may be necessary to move some of them to make the drawing clearer.

Sometimes pipe-run or fitting labels may overlap or obscure other components, making the drawing unclear. These labels should be rearranged. To do this mark the component (e.g. a valve) – the label is highlighted in yellow and an icon () appears. Left-click the icon and drag it to an adequate location. The entire label is moved.

Radiator label may be specified two ways – see section: .