4.10.2. Inserting single fitting components<br>

### 4.10.2. Inserting single fitting components

Fitting components are placed in a similar manner to ordinary components. The difference is that a fitting component must be inserted to an existing component, which we named basic component (for instance pipe-runs).

¨ To insert a fitting component:

1. Make sure that the basic component, onto which fittings will be added, already exists in the project.

2. Click the button representing the required fitting component.

3. As you move the mouse within the project, the outline of the selected component is displayed.

4. Click the basic component into which you want to insert the fitting. The fitting will be inserted only if the fitting component is logically compatible with the basic component.

5. Depending on the set mode of inserting fittings, the component-marking mode is enabled or insertion of another identical fitting is proposed. In the latter case, if you want to abandon inserting fittings, press the right mouse button. Configuration of the mode of inserting fittings is described in section 7.3.1.

! Always click on the component (fragment of the system under design), onto which you want to install the fitting.

! This is of particular importance when a radiator coupling is inserted, which in the drawing is beside the radiator. Logically it forms part of the radiator and space for drawing the radiator coupling will be located automatically. The sequence will look like this:

During inserting After insertion