9.8.4. Radiator heating – radiators sized for an apartment are of different heights<br>

### 9.8.4. Radiator heating – radiators sized for an apartment are of different heights

The method of sizing convectors applied in the program is in large part based on data on the building structure, such as dimensions of recesses under windows. This, however, requires that observing dimension restrictions be enabled. Therefore, if we expect that convectors of the same height are sized for an apartment, and these convectors are placed under windows in the plan view, then we have to make sure that the “Fit to recess” option is enabled. Then convectors will be sized in such manner as to fill in to maximum extent the recess under window, the height of which (more precisely – the elevation of window sill) is the same for the entire storey. Alternatively we can specify the same height for all convectors, using a value taken from the catalogue.