4.10.3. Deleting fitting components<br>

### 4.10.3. Deleting fitting components

To delete a fitting or hardware component you first have to select (mark) it. Therefore, when selecting fitting or hardware components for deletion, always observe messages in the status line to be sure not to select and delete the basic component on which the fitting or hardware is placed.

Remember, that when you delete a basic component that includes fittings, those fittings will also be deleted. You can always undo a delete operation (see section 4.7).