2.3.9. Repeated data diagnostics and analysis of results<br>

### 2.3.9. Repeated data diagnostics and analysis of results

After implementing changes in data you have to do calculations again. The process is the same as described before with the same stages: results of diagnostic run, supply temperature amending – if necessary, analysis of calculation results and changes in pipe spacing.

Amendments must be made until calculation results show no errors and all manifolds are balanced. Then the results are complete and you can proceed to the next stage.