A.1. KEYBOARD<br>

A.1. KEYBOARD

Keys combination: | Operation called in tabular editor:
F1 | opens the graphical catalogue of heaters
| opens the program help
F3 | searching of building material according to entered name.
F4 | opens a pop-up list, for example of defined partitions, partitions orientation etc. in columns of partition table having the same pop-up list
F7 | enables adding of new building material in materials edition window.
| depending on location of project edition, enables adding of new elements of building structure, for example adding of definition of partition, compartment, partition, storey, etc.
F9 | automatic switching to Instal-therm program, function “Area measurement”
F8 | this command generates in window of building materials edition a new material group. This command is only active in a group view of building materials.
| opening/closing of error list window
F12 | calculates the project

Ctrl+F7 | enables adding of a subordinate element of building structure towards the superior, currently selected one, for example adding of new compartment in currently selected flat, partition in selected compartment, etc.
| enables adding and assigning of window/door to partition. That are partitions nested in selected partition.
| in position “Assigning to thermal zones” enables assigning of selected compartment to inserted thermal zone
Ctrl+C | enables copying of selected element (elements) of building structure.
Ctrl+X | enables cutting of selected element (elements) of building structure.
Ctrl+V | enables pasting of copied or cut element of building structure to selected place of the same or another project.
Ctrl+F | switching to window of building materials edition.
Ctrl+G | switching between windows of partition edition and compartment edition.
| this command causes selecting in building structure tree a partition, which have been chosen from compartment table and displaying its edition window.
Ctrl+N | this command is used for creating of new file
Ctrl+O | this command is used for opening of project file, which has been previously saved to disc
Ctrl+P | this command is used for printing of calculations results on a printer.
Ctrl+S | this command causes saving to disc current data in file with current name.
Ctrl+Del | causes deleting of selected element of program data, such as partitions definitions, compartment, flat, etc.
Ctrl+Enter | causes opening of window containing library of building materials.
| causes opening of selection list, for example of defined partitions, partitions orientation, etc. in columns of partitions table, which have such pop-up list.
| enables moving to the next description line, which can be entered in fields concerning project, designer and investor
Ctrl+Space | calling in edition field the numerical data, functions list and expressions variables, which have been pre-defined in program or by the User.
pressed key Ctrl | selecting of several flats with simultaneously pressed Ctrl key allows activation of command enabling connection of flats in one multi-storey flat.
| selecting of chosen elements of program – clicking with pressed Ctrl key will open the multiselect mode.
Ctrl+Alt+Insert | enables entering of expressions variables in any window of project data edition.
Ctrl+<underlined letter> | calling of specified command from main menu of the program.
Enter | confirmation and selection of marked field
Ins | adds program elements, for examples layers, partition definitions in area selected by the cursor, both in edition tables and in „tree” structure of project data.
Shift+<arrows> | selecting of elements of the same type, both in edition tables and in „tree” structure of project data.
| selecting of chosen elements with Shift key will open the multiselect mode.
<arrows> | switching between layers and between columns in partitions table.
| opening the data structure tree to any level
Tab | switching between fields in windows of data edition.
Tab+Shift | switching back between fields in windows of data edition.