A.1. Keyboard:<br>

A.1. Keyboard:

Key combination: | Operation executed:
Esc | refresh display on screen.
F1: | when a component is marked – displays help specific to that component.
| when a component type is being selected from a list – displays help specific to that type.
| when no component is marked – displays general help screen.
| in the error list and in the diagnostics results window – displays information about errors.
F2 | repeat the last value entered in data table.
Shift+F2 | check connections.
F3 | insert the same component/module used last time.
Shift+F3 | pipe-runs re-numbering.
F4 | toggle display: calculated/not calculated installation.
F5 | show the entire project – scale and position are set to display the entire project on the screen.
Shift+F5 | display the entire active layer – set the scale and position to display all components in the active layer.
F7 | project general data – display ”Project options” window on the ”General data” tab.
Ctrl+F7 | building structure - display ”Project options” window on the ”Building structure” tab.
Shift+F7 | project info - display ”Project options” window on the ”Info” tab.
F8 | toggle on/off error list.
Shift+F8 | toggle on/off building structure tree.
F9 | toggle on/off data set list.
Shift+F9 | display toolbar list.
F10 | run calculations.
Shift+F10 | run quick calculations without displaying options and tables.
F11 | toggle on/off table of results in the graphical editor.
F12 | toggle on/off data table.
Alt+C | toggle on/off GRID mode – components snapped to grid.
Alt+Q | display pop-up menu.
Alt+V | toggle on/off AUTO mode – automatic display of possible component connection points.
Alt+X | toggle on/off LOCK mode – lock (protect against moving) all components.
Alt+Z | toggle on/off ORTO mode – place vertical and horizontal components only + optional defined angle.
Alt+B | włączenie/wyłączenie trybu POWT – powtarzalne wstawianie elementów konstrukcji, instalacji i armatury.
Ctrl+A | mark all components in the active layer.
Ctrl+Shift+A | automatically connect marked terminal units.
Ctrl+B | lock (protect against moving) marked components.
Ctrl+C | copy marked components to clipboard.
Ctrl+Shift+C | copy and configure (option) marked elements.
Ctrl+D | unlock marked components – moving enabled.
Ctrl+F | toggle on/off search window.
Ctrl+G | group marked components.
Ctrl+H | ungroup marked components.
Ctrl+I | import plan view from DWG/DXF file.
Ctrl+L | display shortcuts editing window.
Ctrl+M | display macro editing window.
Ctrl+P | print current project section.
Ctrl+Q | divide elements.
Ctrl+R | disconnect marked elements.
Ctrl+Shift+R | completely disconnect marked elements.
Ctrl+S | save project to disk.
Ctrl+V | paste fragment of project or module from clipboard.
Ctrl+X | move marked components to clipboard.
Ctrl+Z | undo last operation.
Ctrl+Y | redo last operation.
Ctrl+Enter | in data table – open a list in a field when available.
Ctrl+Ins | copy marked components to clipboard.
Ctrl+Page Up | toggle to previous worksheet (toggle ”left” among tabs).
Ctrl+Page Down | toggle to next worksheet (toggle ”right” among tabs).
Ctrl+Tab | rotate marked elements horizontally.
Ctrl+„+” | zoom in.
Ctrl+„-” | zoom out.
Ctrl+„*” | enable zoom in.
Ctrl+„/” | enable realtime zoom.
Ctrl+ arrows (arrows pad) | move in specified direction to same type component nearest the marked component.
Ctrl+Alt+ arrows (arrows pad) | move in specified direction to a component of any type nearest the marked component.
Ctrl+ arrows (numerical pad) | move in specified direction to connected component.
Ctrl+Shift+Alt+arrows | duplicate marked fragment of project in specified direction.
Shift+Ins | paste module from clipboard.
Delete | delete marked components.
Enter |