8.4.7. Result editing options<br>

### 8.4.7. Result editing options

Result editing options have no effect on calculations and their results. They only specify the range of generated tables and lists and their editing. They have no effect on the graphical presentation of results.

The result editing options include the following fields:

- Generate bill of mat. – indicate whether the bill of materials is to be drawn up. Disabling this option may shorten the time taken by calculations of large systems on slower computers, when various variants are calculated and the bill of materials will be generated after accepting other results.

- Show integrated valves – indicate whether a list of integrated valves is to be drawn up. May be useful when integrated radiators are used with integrated valves ordered separately.

- Show existing components: With planned, Separately, Disregard – indicate whether components of the “Existing” status (set in data table of the component) are to be displayed in separate list tables, displayed together with components of the “Under design” status or not displayed in lists at all.

- Create lists of components on pipe-runs – indicate whether auxiliary tables titled “List of components on pipe-runs” - showing the components, including all couplings and pipe fittings, installed on individual pipe-runs - are to be generated. Creation of such tables takes up some time and computer power.

- Create lists of components on pipe-runs – indicate whether auxiliary tables titled “List of components on terminal units” - showing the components, including integrated valves and couplings, installed on individual terminal units - are to be generated. Creation of such tables takes up some time and computer power.

- Radiator valves in results table together with radiators – indicate that information on type and setting of an integrated valve and/or integrated coupling is displayed in the terminal units table immediately under the respective radiator. Otherwise a separate table is generated below the terminal units table.