2.4.5. Associating radiators and pipe-runs (originals – shadows)<br>

### 2.4.5. Associating radiators and pipe-runs (originals – shadows)

If system components drawn in the plan views have not been designated as shadows yet, then this has to be done now. Select “Associate original-shadow pairs” in the “Component data” menu. Two windows for editing are opened in which separate sheets may be selected for further operations. By default the current sheet is opened in the left window.

Open the schematic view sheet in one of the windows and the plan view with the shadows in the other window. Now mark a component in one window by clicking on it and mark the corresponding component in the second window in the same manner and click on the “Link” button to effect an association.

Navigation capabilities of the windows used for indicating components are similar to those of the main editing window: zooming in and out, grabber hand for moving the view.

Revoking an association is done by clicking on the shadow component and selecting “Unmark as shadow” from the pop-up menu.