1.1.3. Program calculations results<br>

### 1.1.3. Program calculations results

The most important calculation results are given directly in working tables of individual objects (partitions, compartments) and in cumulative tables with various layout and information. Moreover, in Instal-therm program you can see also the calculation results of heat losses and reduced heat losses in compartments, which are indispensable for further calculations of heating system.

Results have been grouped according to guidelines included in general rules of European Norm or in national appendices to European Norm.

General data include Information concerning project name and general data of building. That are among others data concerning building parameters and general data of building, its dimensions, climatic data, ground.

Results for a building contain results statements for a building concerning the value of coefficients of heat loss by penetration, total heat loss for ventilation, heat energy demand of a building and building features.

Compartments parameters include their temperature, minimal multiplication factor of air exchanges and heating time for all compartments entered in project.

Matching of compartment losses includes compartments listed in a table with values of all heat losses characteristic for compartments.

Compartments results present for each compartment declared in project its belonging to a flat, temperature, dimensions, data of ground, on which the building is located, parameters of additional thermal power, data matching of partitions of a compartment as well as results of heat loss by penetration, ventilation, total net losses and additional heat losses.

Results for partitions concern all partitions defined in project and includes such results as heat penetration coefficient, description, heat flow direction, partition type, value of heat transfer of other and outer part of partition. In case of declaring of laminar partition, additionally the layer structure of partition and chart of temperature drop on these partition layers is presented. Also for defined inhomogeneous partitions some data concerning their names, description, values of heat transfer coefficient and heat penetration resistance on internal and external side are displayed.

Matching of heaters includes selection data as number of compartment, in which the heater has been installed, symbol of heater, temperature in compartment, required heat loss, value of heating agent flow, supply and return temperature, selected type of heater and its dimensions.

The legend includes text description for all symbols appearing in program.