3.4.4. “Building structure” tab<br>

### 3.4.4. “Building structure” tab

The “Building structure” tab is provided for reviewing and editing these building structure data that cannot be accessed via graphical editing. After importing or drawing a plan view of a storey, rooms are created in the graphical editor. These are listed in a “tree” on the left-hand side of the tab. The storey and room components designated with a symbol are graphical components. You can add components of the building by pressing the right mouse button or clicking on the buttons in the upper part of the window. The added components will be marked with a symbol, meaning that they are of tabular type and cannot be displayed on the drawing of the structure. You can, for instance, import or draw the plan views of the ground and first floors – these will form graphical components – and add the attic storey in a tabular form.

! It is not possible to delete graphical components in the building structure tree

The right side of the tab window displays data of the currently marked component. You can enter data for the room (name, comment, heat demand, method of heating and its share in meeting the specified heat demand) and for the apartment and storey (name, comment, storey elevation, storey height, floor thickness, etc.)