4.5.4. Window of partition edition<br>

### 4.5.4. Window of partition edition

Partitions data can be completed in window of compartment edition in partitions table or in partition edition window. To switch between these windows just use the key combination Ctrl+G.

The window of partitions edition can be opened by the User analogous to window of edition of storey, flat and compartment. So, after selecting of chosen partition in building structure tree a window of partition edition „Building structure: Partition” will appear on the right side.

Edition fields contain all partition data required for calculations of heat losses and seasonal energy demand (if such calculations option has been selected).

These fields can be partially completed for partitions defined in “Partitions definitions”, not completed for new entered partitions in compartment or completed according to data entered in partitions table in window of compartment edition. Window of partition edition contains the same fields concerning partitions data as compartment edition window. The User can switch between these windows by means of keys Ctrl+G „Edit partition in compartment view”. For this reason completion of partitions data in selected edition window will cause their completion in corresponding fields.

Partitions data can be completed by the User in fields, the description and meaning of which have been already described in chapter 4.5.3.2. Type of fields present in window of partition edition depends on the type of declared partitions.

Operations available in building structure tree – level of partitions:

Handy menu:

- Add partition F7 – inserts partition as last on the list of partitions of compartment in building structure tree,

- Add partition in cursor’s position Ins – inserts new (next) partition in partitions table in cursor’s position,

- Delete partition (partitions) Ctrl+Del – deletes selected partition (partitions).

- Assign compartment on the other side – for internal partitions causes calling of tree of compartments, which can be adjacent to selected internal partition. Such declared partition is assigned and visible for two adjacent compartments.

- Add partition from adjacent compartment – enables adding of internal, not assigned partition to adjacent compartment. The User can select an adequate internal partition – wall, ceiling, window or internal door from a pop-up tree. Such declared partition is assigned and visible for two adjacent compartments.

- Add partition from adjacent compartment in selected area – enables adding of internal, not assigned partition to adjacent compartment in selected place of building structure tree. . The User can select an adequate internal partition – wall, ceiling, window or internal door from a pop-up tree. Such declared partition is assigned and visible for two adjacent compartments.

- Add window/door Ctrl+F7 – inserts window/door as a nested partition – assigned to external or internal partition. Assigning concerns a nested partition, which shows the icon at this partition.

- Find element in tree/error list – clicking this command will cause finding of selected element, for example storey, flat in displayed error list. In this way the User knows which data have not been completed or have been completed incorrectly.

- Go to partition definition – a command available for partitions defined in “Partitions definitions”. Selecting a chosen partition and selecting this command will cause switching to edition fields in “Partitions definitions”.

- Find compartment in Instal-therm – causes finding of selected compartment in Instal-therm. To make this command active, both programs must be simultaneously opened on the same project. This command enables fast co-operation and communication between programs.

- Copy (Ctrl+C) - copying of selected compartment within building structure of currently edited project to another project.

- Cut (Ctrl+X) – cutting of selected compartment.

- Paste (Ctrl+V) – pasting of copied or cut compartment to selected area of building structure of the same or another project.